# Class MifareUltralight

java.lang.Object
com.codename1.nfc.TagTechnology
com.codename1.nfc.MifareUltralight

public class MifareUltralight extends TagTechnology

NXP MIFARE Ultralight / Ultralight C / NTAG21x technology view. Page-level read/write of 4-byte pages.

Supported on Android (`MifareUltralight`) and iOS 13+ (subset of `NFCMiFareTag`).

- ## Constructor Summary

  Constructors
  Constructor
  Description
  `MifareUltralight()`

- ## Method Summary

  Modifier and Type
  Method
  Description
  `int`
  `getPageCount()`
  Number of pages on this tag.
  `final TagType`
  `getType()`
  The technology variant this view represents.
  `AsyncResource<byte[]>`
  `readPages(int firstPage)`
  Reads 4 pages (16 bytes) starting at `firstPage`.
  `AsyncResource<Boolean>`
  `writePage(int page, byte[] data)`
  Writes a single 4-byte page.

  ### Methods inherited from class TagTechnology

  `transceive`

  ### Methods inherited from class Object

  `clone, equals, getClass, hashCode, notify, notifyAll, toString, wait, wait, wait`

- ## Constructor Details

  - ### MifareUltralight

    public MifareUltralight()

- ## Method Details

  - ### getPageCount

    public int getPageCount()
    Number of pages on this tag. 16 for Ultralight, 48 for Ultralight C, 45 for NTAG213, 135 for NTAG215, 231 for NTAG216. Returns `0` when the port has not populated this field.

  - ### readPages

    public AsyncResource<byte[]> readPages(int firstPage)
    Reads 4 pages (16 bytes) starting at `firstPage`. Pages roll over to page 0 when the request runs past the end.

  - ### writePage

    public AsyncResource<Boolean> writePage(int page, byte[] data)
    Writes a single 4-byte page. Fails with `NfcError.READ_ONLY` for vendor / OTP / lock pages.

  - ### getType

    public final TagType getType()
    Description copied from class: `TagTechnology`
    The technology variant this view represents.
    Specified by:
      `getType` in class `TagTechnology`